Connection point 3ph+N+E, 380 volts, 16 Amps, CEE type "female" connector (maximum power is 10 kW)

16 A

Connection point 3ph+N+E, 380 volts, 32 Amps, CEE type "female" connector (maximum power is 20 kW)

32 A

Connection point 3ph+N+E, 380 volts, 63 Amps, CEE type "female" connector (maximum power is 40 kW)

63 A

Connection point 3ph+N+E, 380 volts, 125 Amps, CEE type "female" connector (maximum power is 80 kW)

125 A

Connection point 1ph+N+E, 230 volt, 16 Amps, CEE type "female" connector (maximum power is 2 kW)

16 A

Connection point 1ph+N+E, 230 volt, 32 Amps, CEE type "female" connector (maximum power is 5 kW)

32 A

Connection point 1ph+N+E, 230 volt, 10 Amps, Schuko type "EU" connector (maximum power is 2 kW)



Suspension point is 50 kg.

50

Suspension point is 100 kg.

100

Suspension point is 250 kg.

250

Suspension point is 320 kg.

320

Suspension point is 500 kg.

500

Suspension point is 1,000 kg.

1000

\* points with a guy rope cannot be less than 100 kg